Back to Contents

# Specifications

This section provides specification information for the family of Intel® wireless adapters. The following list may not be all inclusive.

- Intel® Dual Band Wireless-AC 3165
- Intel® Dual Band Wireless-AC 3168
- Intel® Dual Band Wireless-AC 7265
- Intel® Dual Band Wireless-N 7265
- Intel® Wireless-N 7265
- Intel® Dual Band Wireless-AC 8260
- Intel® Dual Band Wireless-AC 8265
- Intel® Wireless-AC 9260
- Intel® Wireless-AC 9461
- Intel® Wireless-AC 9462
- Intel® Wireless-AC 9560
- Intel® Wi-Fi 6 AX101
- Intel® Wi-Fi 6 AX200
- Intel® Wi-Fi 6 AX201
- Intel® Wi-Fi 6 AX203
- Intel® Wi-Fi 6E AX210
- Intel® Wi-Fi 6E AX211
- Intel® Wi-Fi 6E AX411
- Intel® Wi-Fi 7 BE200
- Intel® Wi-Fi 7 BE201
- Intel® Wi-Fi 7 BE202
- Intel® Wi-Fi 7 BE211
- Intel® Wi-Fi 7 BE213

## Intel® Dual Band Wireless-AC 3165 (Model 3165NGW)

Form Factors | M.2 (Next Generation Form Factor - NGFF)
Electrical interfaces | PCIe and USB 2.0
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | 802.11abgn, 802.11ac, 802.11d, 802.11e, 802.11i, 802.11h, 802.11w
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
Spatial streams | Intel® Dual Band Wireless-AC 3165: 1 X 1
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | Intel® Dual Band Wireless-AC 3165: Up to 433 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Dual Mode Bluetooth* 2.1, 2.1+EDR, 3.0, 3.0+HS, 4.0 (BLE)
General
Operating Systems | Windows* 7 (32-bit and 64-bit), Windows* 8 (32-bit and 64-bit), Windows* 8.1 (64-bit)
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* for 802.11ac, a/b/g, n, WMM*, WPA*, WPA2*, and WPS, WPS 2.0, Protected Management Frames. Wi-Fi Direct* for peer-to-peer device connections.
Architecture | Infrastructure and SoftAP; Supports simultaneous Client and SoftAP modes
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, AES-CCMP, TKIP
Wi-Fi Direct* Encryption and Authentication | WPA2, AES-CCMP
Product Safety | UL, C-UL, CB (IEC/EN 62368-1)

## Intel® Dual Band Wireless-AC 3168

Form Factors | M.2 2230 (Next Generation Form Factor - NGFF)
Electrical interfaces | PCIe and USB 2.0
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | 802.11abgn, 802.11ac, 802.11d, 802.11e, 802.11i, 802.11h, 802.11w
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
Spatial streams | Intel® Dual Band Wireless-AC 3168: 1 X 1
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | Intel® Dual Band Wireless-AC 3168: Up to 433 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Dual Mode Bluetooth* 2.1, 2.1+EDR, 3.0, 3.0+HS, 4.2 (BLE)
General
Operating Systems | Linux, Windows* 8.1 (64-bit), Windows* 10 (64-bit)
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* for 802.11ac, a/b/g, n, WMM*, WPA*, WPA2*, and WPS, WPS 2.0, Protected Management Frames. Wi-Fi Direct* for peer-to-peer device connections.
Architecture | Infrastructure and SoftAP; Supports simultaneous Client and SoftAP modes
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, AES-CCMP, TKIP
Wi-Fi Direct* Encryption and Authentication | WPA2, AES-CCMP
Product Safety | UL, C-UL, CB (IEC/EN 62368-1)

## Intel® Dual Band Wireless-AC 7265 (Model 7265NGW)

Form Factors | M.2 (Next Generation Form Factor - NGFF)
Electrical interfaces | PCIe and USB 2.0
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | Intel® Dual Band Wireless-AC 7265 Model 7265NGW - 802.11agn, ac, 2x2, Bluetooth 4.0, PCIe, USB, M.2
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
Spatial streams | Intel® Dual Band Wireless-AC 7265: 2 X 2
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | Intel® Dual Band Wireless-AC 7265: Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Dual Mode Bluetooth* 2.1, 2.1+EDR, 3.0, 3.0+HS, 4.0 (BLE) supported by the following adapters Model 7265NGW
General
Operating Systems | Windows* 7 (32-bit and 64-bit), Windows* 8 (32-bit and 64-bit), Windows* 8.1 (64-bit)
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* for 802.11ac, a/b/g, n, WMM*, WPA*, WPA2*, and WPS, WPS 2.0, Protected Management Frames. Wi-Fi Direct* for peer-to-peer device connections.
Architecture | Infrastructure and SoftAP; Supports simultaneous Client and SoftAP modes
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, AES-CCMP, TKIP
Wi-Fi Direct* Encryption and Authentication | WPA2, AES-CCMP
Product Safety | UL, C-UL, CB (IEC/EN 62368-1)

## Intel® Dual Band Wireless-N 7265 (Models 7265NGW AN and 7265NGW NB)
Intel® Wireless-N 7265 (Model 7265NGW BN)

Form Factors | M.2 (Next Generation Form Factor - NGFF)
Electrical interfaces | PCIe, USB 2.0
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | Intel® Dual Band Wireless-N 7265 Model 7265NGW AN - 802.11agn, 2x2, Bluetooth 4.0, PCIe, USB, M.2 Model 7265NGW NB - 802.11agn, 2x2, PCIe, USB, M.2 Intel® Wireless-N 7265 Model 7265NGW BN - 802.11bgn, 2x2, Bluetooth 4.0, PCIe, USB, M.2
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 90% non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation (See above, not all bands supported by all adapters) | 5GHz (802.11a/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
802.11n spatial streams | All adapters: 2 X 2 spatial streams
Data Rates | All data rates are theoretical maximums.
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Dual Mode Bluetooth* 2.1, 2.1+EDR, 3.0, 3.0+HS, 4.0 (BLE) supported by the following adapters Model 7265NGW AN Model 7265NGW NB Model 7265NGW BN
General
Operating Systems | Windows* 7 (32-bit and 64-bit), Windows 8 (32-bit and 64-bit), Windows* 8.1 (64-bit)
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* for 802.11ac, a/b/g, n, WMM*, WPA*, WPA2*, and WPS, WPS 2.0, Protected Management Frames. Wi-Fi Direct* for peer-to-peer device connections.
Architecture | Infrastructure and SoftAP; Supports simultaneous Client and SoftAP modes
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, AES-CCMP, TKIP
Wi-Fi Direct* Encryption and Authentication | WPA2, AES-CCMP
Product Safety | UL, C-UL, CB (IEC/EN 62368-1)

## Intel® Dual Band Wireless-AC 8260

Form Factors | Half-Mini Card and M.2 (Next Generation Form Factor - NGFF)
Electrical interfaces | PCIe and USB 2.0 for both form factors
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
IEEE 802.11 Networking Standards | Intel® Dual Band Wireless-AC 8260 Model 8260NGW - 802.11agn, ac, 2x2, Bluetooth 4.0, PCIe, USB, M.2
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 95% non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
Spatial streams | Intel® Dual Band Wireless-AC 8260: 2 X 2
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | Intel® Dual Band Wireless-AC 8260: Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
Bluetooth | Dual Mode Bluetooth* 2.1, 2.1+EDR, 3.0, 3.0+HS, 4.0 (BLE) supported by the following adapters Model 8260NGW
General
Operating Systems | Windows* 7 (32-bit and 64-bit), Windows* 8 (32-bit and 64-bit), Windows* 8.1 (64-bit)
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* for 802.11ac, a/b/g, n, WMM*, WPA*, WPA2*, and WPS, WPS 2.0, Protected Management Frames. Wi-Fi Direct* for peer-to-peer device connections.
Architecture | Infrastructure and SoftAP; Supports simultaneous Client and SoftAP modes
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, AES-CCMP, TKIP
Wi-Fi Direct* Encryption and Authentication | WPA2, AES-CCMP
Product Safety | UL, C-UL, CB (IEC/EN 62368-1)

## Intel® Dual Band Wireless-AC 8265 (Models 8265NGWH/8265NGW/8265D2W)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.4 mm M.2 1216: 12 mm x 16 mm x 1.8 mm
Weight | M.2 2230: 2.6g M.2 1216: 0.6g
Antenna Diversity | Supported
Radio ON/OFF Control | Supported
Connector Interface | M.2: PCIe, USB, or UART (M.2 1216 only)
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 ºC to 35 ºC)
Operating Systems | Microsoft Windows 7*, Microsoft Windows 8.1*, Microsoft Windows 10*, Linux* (limited feature support), Android
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* a/b/g/n/ac, WMM*, WMM-PS*, WPA*, WPA2*, WPS2*, Protected Management Frames, Wi-Fi Direct* for peer to peer device connections, Wi-Fi Miracast* as Source.
IEEE WLAN Standard | IEEE 802.11a/b/g/n/ac, 802.11d, 802.11e, 802.11h, 802.11i, 802.11w; 802.11r, 802.11k, 802.11v pending OS support; Fine Timing Measurement based on 802.11REVmc
Roaming | Supports seamless roaming between access points
Bluetooth | Dual Mode Bluetooth* 4.2, BLE
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, LEAP, EAP-FAST), EAP-SIM, EAP-AKA, EAP-AKA
Authentication Protocols | PAP, CHAP, TLS, GTC, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, 128-bit AES-CCMP
Wi-Fi Direct* Encryption and Authentication | WPA2-PSK, AES-CCMP
Compliance
Product Safety | UL, C-UL, CB (IEC 62368-1)
Model Numbers
Models | Model 8265NGWH | 802.11ac, 2x2, Bluetooth* 4.2, PCIe, USB, LTE Coexistence, eFEM, M.2 2230 HE
Model 8265NGW | 802.11ac, 2x2, Bluetooth* 4.2, PCIe, USB, M.2 2230 MS
Model 8265D2W | 802.11ac, 2x2, Bluetooth* 4.2, PCIe, LTE Coexistence, M.2 1216 SD
Frequency Modulation | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
Spatial streams | Intel® Dual Band Wireless-AC 8265: 2 X 2
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | Intel® Dual Band Wireless-AC 8265: Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps

## Intel® Wireless-AC 9260 (Models 9260NGW and 9260D2WL)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.4 mm [1.5 mm max (top side)/ 0.1 mm max (bottom side)] M.2 1216: 12 mm x 16 mm x 1.67 (±0.08) mm
Weight | M.2 2230: 2.9 ±0.3 g M.2 1216: 0.61 ±0.1 g
Antenna Diversity | Supported
Radio ON/OFF Control | Supported
Connector Interface | M.2: PCIe, USB
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 ºC to 35 ºC)
Operating Systems | Microsoft Windows 10*, Linux* (limited feature support), Chrome*
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* a/b/g/n/ac with wave 2 features, WMM*, WMM-PS*, WPA*, WPA2*, WPS2*, Protected Management Frames, Wi-Fi Miracast* as Source, and Wi-Fi Direct*.
IEEE WLAN Standard | IEEE 802.11a/b/g/n/ac, 802.11d, 802.11e, 802.11h, 802.11i, 802.11w; 802.11r, 802.11k, 802.11v pending OS support; Fine Timing Measurement based on 802.11REVmc
Roaming | Supports seamless roaming between access points
Bluetooth | Bluetooth* 5
Security
Authentication | WPA* and WPA2*, 802.1X (EAP-TLS, TTLS, PEAP, EAP-SIM, EAP-AKA, EAP-AKA)
Authentication Protocols | PAP, CHAP, TLS, MS-CHAP*, MS-CHAPv2*
Encryption | 64-bit and 128-bit WEP, 128-bit AES-CCMP
Wi-Fi Direct* Encryption and Authentication | WPA2-PSK, AES-CCMP
Compliance
US Government | FIPS, FISMA
Product Safety | UL, C-UL, CB (IEC 62368-1)
Model Numbers
Models | 9260NGW | 802.11ac wave 2, 2x2, Bluetooth* 5, PCIe, USB, M.2 2230
9260D2WL | 802.11ac wave 2, 2x2, Bluetooth* 5, PCIe, USB, M.2 1216 LTE Coex
Frequency Modulation | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
Spatial streams | Intel® Wireless-AC 9260: 2 X 2
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | 1.73 Gbps when using 160MHz channels
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps

## Intel® Wireless-AC 9461 (Models 9461NGW/9461D2W)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.4 mm M.2 1216: 12 mm x 16 mm x 1.57 (+-0.08) mm
Weight | M.2 2230: 2.7g M.2 1216: 0.7g
Antenna Diversity | Supported
Radio ON/OFF Control | Supported
Connector Interface | M.2: CNVio
Operating Temperature (Adapter Shield) | 0ºC to +80ºC
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 ºC to 35 ºC)
Operating Systems | Microsoft Windows 10*, Linux* (limited feature support), Chrome
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* a/b/g/n/ac with wave 2 features, WMM*, WMM-PS*, WPA*, WPA2*, WPS2*, Protected Management Frames, Wi-Fi Miracast* as Source, and Wi-Fi Direct
IEEE WLAN Standard | IEEE 802.11a/b/g/n/ac, 802.11d, 802.11e, 802.11h, 802.11i, 802.11w; 802.11r, 802.11k, 802.11v pending OS support; Fine Timing Measurement based on 802.11REVmc
Roaming | Supports seamless roaming between access points
Bluetooth | Bluetooth* 5
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, EAP-SIM, EAP-AKA)
Authentication Protocols | PAP, CHAP, TLS, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, 128-bit AES-CCMP
Wi-Fi Direct* Encryption and Authentication | WPA2-PSK, AES-CCMP
Compliance
Regulatory | For a list of country approvals, please contact your local Intel representatives.
US Government | FIPS, FISMA
Product Safety | UL, C-UL, CB (IEC 62368-1)
Model Numbers
Models | 9461NGW | 802.11ac wave 2, 1x1, Bluetooth* 5, PCIe, USB, M.2 2230, Single Antenna
9461D2W | 802.11ac wave 2, 1x1, Bluetooth* 5, PCIe, USB, M.2 1216, Single Antenna
Frequency Modulation | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
Spatial streams | Intel® Wireless-AC 9461: 1 X 1
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | 433 Mbps when using 80MHz channels
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps

## Intel® Wireless-AC 9462 (Models 9462NGW/9462D2W)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.4 mm M.2 1216: 12 mm x 16 mm x 1.57 (+-0.08) mm
Weight | M.2 2230: 2.7g M.2 1216: 0.7g
Antenna Diversity | Supported
Radio ON/OFF Control | Supported
Connector Interface | M.2: CNVio
Operating Temperature (Adapter Shield) | 0ºC to +80ºC
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 ºC to 35 ºC)
Operating Systems | Microsoft Windows 10*, Linux* (limited feature support), Chrome
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* a/b/g/n/ac with wave 2 features, WMM*, WMM-PS*, WPA*, WPA2*, WPS2*, Protected Management Frames, Wi-Fi Miracast* as Source, and Wi-Fi Direct
IEEE WLAN Standard | IEEE 802.11a/b/g/n/ac, 802.11d, 802.11e, 802.11h, 802.11i, 802.11w; 802.11r, 802.11k, 802.11v pending OS support; Fine Timing Measurement based on 802.11REVmc
Roaming | Supports seamless roaming between access points
Bluetooth | Bluetooth* 5
Security
Authentication | WPA and WPA2, 802.1X (EAP-TLS, TTLS, PEAP, EAP-SIM, EAP-AKA)
Authentication Protocols | PAP, CHAP, TLS, MS-CHAP*, MS-CHAPv2
Encryption | 64-bit and 128-bit WEP, 128-bit AES-CCMP
Wi-Fi Direct* Encryption and Authentication | WPA2-PSK, AES-CCMP
Compliance
Regulatory | For a list of country approvals, please contact your local Intel representatives.
US Government | FIPS, FISMA
Product Safety | UL, C-UL, CB (IEC 62368-1)
Model Numbers
Models | 9462NGW | 802.11ac wave 2, 1x1, Bluetooth* 5, PCIe, USB, M.2 2230, Diversity Antenna
9462D2W | 802.11ac wave 2, 1x1, Bluetooth* 5, PCIe, USB, M.2 1216, Diversity Antenna
Frequency Modulation | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
Spatial streams | Intel® Wireless-AC 9462: 1 X 1
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | 433 Mbps when using 80MHz channels
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps

## Intel® Wireless-AC 9560 (Models 9560NGW/9560D2W)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.4 mm M.2 1216: 12 mm x 16 mm x 1.8 mm
Weight | M.2 2230: 2.6g M.2 1216: 0.6g
Antenna Diversity | Supported
Radio ON/OFF Control | Supported
Connector Interface | M.2: CNVio
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 ºC to 35 ºC)
Operating Systems | Microsoft Windows 10*, Linux* (limited feature support), Chrome*
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* a/b/g/n/ac with wave 2 features, WMM*, WMM-PS*, WPA*, WPA2*, WPS2*, Protected Management Frames, Wi-Fi Miracast* as Source, and Wi-Fi Direct* (For Microsoft Windows* only).
IEEE WLAN Standard | IEEE 802.11a/b/g/n/ac, 802.11d, 802.11e, 802.11h, 802.11i, 802.11w; 802.11r, 802.11k, 802.11v pending OS support; Fine Timing Measurement based on 802.11-2016
Roaming | Supports seamless roaming between access points
Bluetooth | Bluetooth* 5
Security
Authentication | WPA* and WPA2*, 802.1X (EAP-TLS, TTLS, PEAP, EAP-SIM, EAP-AKA, EAP-AKA)
Authentication Protocols | PAP, CHAP, TLS, MS-CHAP*, MS-CHAPv2*
Encryption | 64-bit and 128-bit WEP, 128-bit AES-CCMP
Wi-Fi Direct* Encryption and Authentication | WPA2-PSK, AES-CCMP
Compliance
US Government | FIPS, FISMA
Product Safety | UL, C-UL, CB (IEC 62368-1)
Model Numbers
Models | 9560NGW | 802.11ac wave 2, 2x2, Bluetooth* 5, PCIe, USB, M.2 2230
9560D2W | 802.11ac wave 2, 2x2, Bluetooth* 5, PCIe, USB, M.2 1216
Frequency Modulation | 5GHz (802.11ac/n) | 2.4GHz (802.11b/g/n)
Frequency band | 5.15GHz - 5.85GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | All channels as defined by the relevant specification and country rules.
Spatial streams | Intel® Wireless-AC 9560: 2 X 2
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ac Data Rates | 1.73 Gbps when using 160MHz channels
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps

## Intel® Wi-Fi 6 AX101 (AX101NGW/AX101D2W)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.4 mm [1.5 mm max (top side)/ 0.1 mm max (bottom side)] M.2 1216: 12 mm x 16 mm x 1.65 (±0.05) mm
Weight | M.2 2230: 2.33 (±0.3) g M.2 1216: 0.61 (±0.1) g
Antenna Diversity | Supported
Radio ON/OFF Control | Supported
Connector Interface | M.2: CNVio2
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 °C to 35 °C)
Operating Systems | Microsoft Windows 10*, Linux*, Chrome OS*
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* 6, Wi-Fi CERTIFIED* a/b/g/n/ac, WMM*, WMM-PS*, WPA*, WPA2*, WPA3*, WPS*, PMF*, Wi-Fi Direct*, Wi-Fi Agile Multiband*, Wi-Fi Optimized Connectivity*, Wi-Fi Location*, and Wi-Fi TimeSync*
IEEE WLAN Standard | IEEE 802.11-2016 and select amendments (selected feature coverage) IEEE 802.11a,b,d,e,g,h,i,k,n,r,u,v,w,ac,ax; Fine Timing Measurement based on 802.11-2016
Bluetooth | Bluetooth* 5.1
Security
Authentication | WPA* and WPA2* Personal and Enterprise; WPA3* (pending OS support)
Authentication Protocols | 802.1X EAP-TLS, EAP-TTLS/MSCHAPv2, PEAPv0/EAP-MSCHAPv2 (EAP-SIM, EAP-AKA, EAP-AKA')
Encryption | 64-bit and 128-bit WEP, TKIP, 128-bit AES-CCMP, 256-bit AES-GCMP
Compliance
Regulatory | For a list of country approvals, please contact your local Intel representatives.
US Government | FIPS 140-2
Product Safety | UL, C-UL, CB (IEC 62368-1)
Model Numbers
Models | AX101NGW | Wi-Fi 6 (802.11ax) 1x1 80MHz, Bluetooth* 5.1, M.2 2230, Antenna Diversity
AX101D2W | Wi-Fi 6 (802.11ax) 1x1 80MHz, Bluetooth* 5.1, M.2 1216, Antenna Diversity

## Intel® Wi-Fi 6 AX200 (AX200NGW/AX200D2WL)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.4 mm [1.5 mm max (top side)/ 0.1 mm max (bottom side)] M.2 1216: 12 mm x 16 mm x 1.65 (±0.05) mm
Weight | M.2 2230: 2.33 (±0.3) g M.2 1216: 0.61 (±0.1) g
Antenna Diversity | Supported
Radio ON/OFF Control | Supported
Connector Interface | M.2: PCIe, USB
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 °C to 35 °C)
Operating Systems | Microsoft Windows 10*, Linux*, Chrome OS*
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* a/b/g/n/ac with wave 2 features, WMM*, WMM-PS*, WPA*, WPA2*, WPS*, PMF*, Wi-Fi Direct*, Wi-Fi Miracast*, Wi-Fi Agile Multiband*, Wi-Fi Optimized Connectivity*, Wi-Fi Location*, Passpoint*, Wi-Fi Aware*, and Wi-Fi TimeSync*
IEEE WLAN Standard | IEEE 802.11-2016 and select amendments (selected feature coverage) IEEE 802.11a, b, g, n, ac, ax, d, e, h, i, k, r, u, v, w, ai; Fine Timing Measurement based on 802.11-2016
Bluetooth | Bluetooth* 5
Security
Authentication | WPA* and WPA2* Personal and Enterprise; WPA3* (pending OS support)
Authentication Protocols | 802.1X EAP-TLS, EAP-TTLS/MSCHAPv2, PEAPv0/EAP-MSCHAPv2 (EAP-SIM, EAP-AKA, EAP-AKA')
Encryption | 64-bit and 128-bit WEP, TKIP, 128-bit AES-CCMP, 256-bit AES-GCMP
Compliance
Regulatory | For a list of country approvals, please contact your local Intel representatives.
US Government | FIPS 140-2, FISMA
Product Safety | UL, C-UL, CB (IEC 62368-1)
Model Numbers
Models | AX200NGW | 802.11ax, 2x2, Bluetooth* 5, M.2 2230
AX200D2WL | 802.11ax, 2x2, Bluetooth* 5, M.2 1216; LTE Coexistence
Frequency Modulation | 5GHz (802.11a/n/ac/ax) | 2.4GHz (802.11b/g/n/ax)
Frequency band | 5.15GHz - 5.895GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM | CCK, DQPSK, DBPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiple Access (OFDMA) | 2.4GHz ISM: Orthogonal Frequency Division Multiple Access (OFDMA)
Channels | All channels as defined by the relevant specification and country rules.
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ax Data Rates | Up to 2.4 Gbps
IEEE 802.11ac Data Rates | Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps

## Intel® Wi-Fi 6 AX201 (AX201NGW/AX201D2W/AX201D2WL)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.4 mm [1.5 mm max (top side)/ 0.1 mm max (bottom side)] M.2 1216: 12 mm x 16 mm x 1.65 (±0.05) mm
Weight | M.2 2230: 2.33 (±0.3) g M.2 1216: 0.61 (±0.1) g
Radio ON/OFF Control | Supported
Connector Interface | M.2: CNVio2
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 °C to 35 °C)
Operating Systems | Microsoft Windows 10*, Linux*, Chrome OS*
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* a/b/g/n/ac with wave 2 features, WMM*, WMM-PS*, WPA*, WPA2*, WPS*, PMF*, Wi-Fi Direct*, Wi-Fi Miracast*, Wi-Fi Agile Multiband*, Wi-Fi Optimized Connectivity*, Wi-Fi Location*, Passpoint*, Wi-Fi Aware*, and Wi-Fi TimeSync*
IEEE WLAN Standard | IEEE 802.11-2016 and select amendments (selected feature coverage) IEEE 802.11a, b, g, n, ac, ax, d, e, h, i, k, r, u, v, w, ai; Fine Timing Measurement based on 802.11-2016
Bluetooth | Bluetooth* 5
Security
Authentication | WPA* and WPA2* Personal and Enterprise; WPA3* (pending OS support)
Authentication Protocols | 802.1X EAP-TLS, EAP-TTLS/MSCHAPv2, PEAPv0/EAP-MSCHAPv2 (EAP-SIM, EAP-AKA, EAP-AKA')
Encryption | 64-bit and 128-bit WEP, TKIP, 128-bit AES-CCMP, 256-bit AES-GCMP
Compliance
Regulatory | For a list of country approvals, please contact your local Intel representatives.
US Government | FIPS 140-2, FISMA
Product Safety | UL, C-UL, CB (IEC 62368-1)
Model Numbers
Models | Model AX201NGW | 802.11ax, 2x2, Bluetooth* 5, M.2 2230
AX201D2W | 802.11ax, 2x2, Bluetooth* 5, M.2 1216
AX201D2WL | 802.11ax, 2x2, Bluetooth* 5, M.2 1216; LTE Coexistence
Frequency Modulation | 5GHz (802.11a/n/ac/ax) | 2.4GHz (802.11b/g/n/ax)
Frequency band | 5.15GHz - 5.895GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM | CCK, DQPSK, DBPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM
Wireless Medium | 5GHz UNII: Orthogonal Frequency Division Multiple Access (OFDMA) | 2.4GHz ISM: Orthogonal Frequency Division Multiple Access (OFDMA)
Channels | All channels as defined by the relevant specification and country rules.
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ax Data Rates | Up to 2.4 Gbps
IEEE 802.11ac Data Rates | Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps

## Intel® Wi-Fi 6 AX203 (AX203NGW/AX203D2W)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.4 mm [1.5 mm max (top side)/ 0.1 mm max (bottom side)] M.2 1216: 12 mm x 16 mm x 1.65 (±0.05) mm
Weight | M.2 2230: 2.33 (±0.3) g M.2 1216: 0.61 (±0.1) g
Radio ON/OFF Control | Supported
Connector Interface | M.2: CNVio2
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 °C to 35 °C)
Operating Systems | Microsoft Windows 10*, Linux*, Chrome OS*
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* 6, Wi-Fi CERTIFIED* a/b/g/n/ac, WMM*, WMM-PS*, WPA*, WPA2*, WPA3*, WPS*, PMF*, Wi-Fi Direct*, Wi-Fi Agile Multiband*, Wi-Fi Optimized Connectivity*, Wi-Fi Location*, and Wi-Fi TimeSync*
IEEE WLAN Standard | IEEE 802.11-2016 and select amendments (selected feature coverage) IEEE 802.11a,b,d,e,g,h,i,k,n,r,u,v,w,ac,ax; Fine Timing Measurement based on 802.11-2016
Bluetooth | Bluetooth* 5.1
Security
Authentication | WPA* and WPA2* Personal and Enterprise; WPA3* (pending OS support)
Authentication Protocols | 802.1X EAP-TLS, EAP-TTLS/MSCHAPv2, PEAPv0/EAP-MSCHAPv2 (EAP-SIM, EAP-AKA, EAP-AKA')
Encryption | 64-bit and 128-bit WEP, TKIP, 128-bit AES-CCMP, 256-bit AES-GCMP
Compliance
Regulatory | For a list of country approvals, please contact your local Intel representatives.
US Government | FIPS 140-2
Product Safety | UL, C-UL, CB (IEC 62368-1)
Model Numbers
Models | AX203NGW | Wi-Fi 6 (802.11ax) 2x2 80MHz, Bluetooth* 5.1, M.2 2230
AX203D2W | Wi-Fi 6 (802.11ax) 2x2 80MHz, Bluetooth* 5.1, M.2 1216

## Intel® Wi-Fi 6E AX210 (AX210NGW/AX210D2W)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.4 mm [1.5 mm max (top side)/ 0.1 mm max (bottom side)] M.2 1216: 12 mm x 16 mm x 1.65 (±0.08) mm
Weight | M.2 2230: 2.33 (±0.3) g M.2 1216: 0.61 (±0.1) g
Radio ON/OFF Control | Supported
Connector Interface | M.2: PCIe, USB
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 °C to 35 °C)
Operating Systems | Microsoft Windows 10*, Linux*
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* a/b/g/n/ac, WMM*, WMM-PS*, WPA2*, WPA3*, WPS*, PMF*, Wi-Fi Direct*, Wi-Fi Agile Multiband* and Wi-Fi TimeSync*
IEEE WLAN Standard | IEEE 802.11-2016 and select amendments (selected feature coverage) IEEE 802.11a, b, g, n, ac, ax, d, e, h, i, k, r, u, v, w; Fine Timing Measurement based on 802.11-2016 802.11-2016, Wi-Fi Location R2 (802.11az) HW readiness
Bluetooth | Bluetooth* 5.2
Security
Authentication | WPA2* and WPA3*
Authentication Protocols | 802.1X EAP-TLS, EAP-TTLS/MSCHAPv2, PEAPv0/EAP-MSCHAPv2 (EAP-SIM, EAP-AKA, EAP-AKA')
Encryption | 128-bit AES-CCMP, 256-bit AES-GCMP
Compliance
Regulatory | For a list of country approvals, please contact your local Intel representatives.
US Government | FIPS 140-2
Product Safety | UL, C-UL, CB (IEC 62368-1)
Model Numbers
Models | AX210NGW | Wi-Fi 6E (6GHz), 2x2, Bluetooth* 5.2, M.2 2230
AX210D2W | Wi-Fi 6E (6GHz), 2x2, Bluetooth* 5.2, M.2 1216
Frequency Modulation | 6-7GHz (802.11ax R2) | 5GHz (802.11a/n/ac/ax) | 2.4GHz (802.11b/g/n/ax)
Frequency band | FCC: 5.925GHz-7.125GHz EU: 5925GHz- 6.425GHz (dependent on country) | 5.15GHz - 5.895GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM | CCK, DQPSK, DBPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM
Wireless Medium | 6-7GHz: Orthogonal Frequency Division Multiple Access (OFDMA) | 5GHz UNII: Orthogonal Frequency Division Multiple Access (OFDMA) | 2.4GHz ISM: Orthogonal Frequency Division Multiple Access (OFDMA)
Channels | All channels as defined by the relevant specification and country rules.
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ax Data Rates | Up to 2.4 Gbps
IEEE 802.11ac Data Rates | Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps

## Intel® Wi-Fi 6E AX211 (AX211NGW/AX211D2W/AX211D2WL)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.4 mm [1.5 mm max (top side)/ 0.1 mm max (bottom side)] M.2 1216: 12 mm x 16 mm x 1.7 (±0.1) mm
Weight | M.2 2230: 2.83 (±0.3) g M.2 1216: 0.67 (±0.1) g
Radio ON/OFF Control | Supported
Connector Interface | M.2: CNVio2
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 °C to 35 °C)
Operating Systems | Microsoft Windows 10*, Linux*
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* a/b/g/n/ac, WMM*, WMM-PS*, WPA3*, PMF*, Wi-Fi Direct*, and Wi-Fi Agile Multiband*
IEEE WLAN Standard | IEEE 802.11-2016 and select amendments (selected feature coverage) IEEE 802.11a, b, g, n, ac, ax, d, e, h, i, k, r, u, v, w; Fine Timing Measurement based on 802.11-2016 Wi-Fi Location R2 (802.11az) HW readiness
Bluetooth | Bluetooth* 5.2
Security
Authentication | WPA2* and WPA3*
Authentication Protocols | 802.1X EAP-TLS, EAP-TTLS/MSCHAPv2, PEAPv0/EAP-MSCHAPv2 (EAP-SIM, EAP-AKA, EAP-AKA')
Encryption | 128-bit AES-CCMP, 256-bit AES-GCMP
Compliance
Regulatory | For a list of country approvals, please contact your local Intel representatives.
US Government | FIPS 140-2
Product Safety | UL, C-UL, CB (IEC 62368-1)
Model Numbers
Models | AX211NGW | Wi-Fi 6E (6GHz), 2x2, Bluetooth* 5.2, M.2 2230
AX211D2W | Wi-Fi 6E (6GHz), 2x2, Bluetooth* 5.2, M.2 1216
AX211D2WL | Wi-Fi 6E (6GHz), 2x2, Bluetooth* 5.2, M.2 1216, LTE Coex
Frequency Modulation | 6-7GHz (802.11ax R2) | 5GHz (802.11a/n/ac/ax) | 2.4GHz (802.11b/g/n/ax)
Frequency band | FCC: 5.925GHz-7.125GHz EU: 5925GHz- 6.425GHz (dependent on country) | 5.15GHz - 5.895GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM | CCK, DQPSK, DBPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM
Wireless Medium | 6-7GHz: Orthogonal Frequency Division Multiple Access (OFDMA) | 5GHz UNII: Orthogonal Frequency Division Multiple Access (OFDMA) | 2.4GHz ISM: Orthogonal Frequency Division Multiple Access (OFDMA)
Channels | All channels as defined by the relevant specification and country rules.
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ax Data Rates | Up to 2.4 Gbps
IEEE 802.11ac Data Rates | Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps

## Intel® Wi-Fi 6E AX411 (AX411NGW/AX411E2W)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.4 mm [1.5 mm max (top side)/ 0.1 mm max (bottom side)] M.2 1625: 16 mm x 25 mm x 2.0 mm
Weight | M.2 2230: 2.83 (±0.3) g M.2 1625: 0.90 (±0.1) g
Radio ON/OFF Control | Supported
Connector Interface | M.2: CNVio2
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 °C to 35 °C)
Operating Systems | Microsoft Windows 10*, Linux*
Wi-Fi Alliance* certification | Wi-Fi CERTIFIED* 6, Wi-Fi CERTIFIED* a/b/g/n/ac, WMM*, WMM-PS*, WPA3*, PMF*, Wi-Fi Direct*, and Wi-Fi Agile Multiband*
IEEE WLAN Standard | IEEE 802.11-2016 and select amendments (selected feature coverage) IEEE 802.11a, b, g, n, ac, ax, d, e, h, i, k, r, u, v, w; Fine Timing Measurement based on 802.11-2016 Wi-Fi Location R2 (802.11az) HW readiness
Bluetooth | Bluetooth* 5.2
Security
Authentication | WPA2* and WPA3*
Authentication Protocols | 802.1X EAP-TLS, EAP-TTLS/MSCHAPv2, PEAPv0/EAP-MSCHAPv2 (EAP-SIM, EAP-AKA, EAP-AKA')
Encryption | 128-bit AES-CCMP, 256-bit AES-GCMP
Compliance
Regulatory | For a list of country approvals, please contact your local Intel representatives.
US Government | FIPS 140-2
Product Safety | UL, C-UL, CB (IEC 62368-1)
Model Numbers
Models | AX411NGW | Wi-Fi 6E (6GHz), 2x2, Bluetooth* 5.2, M.2 2230
AX411E2W | Wi-Fi 6E (6GHz), 2x2, Bluetooth* 5.2, M.2 1625
Frequency Modulation | 6-7GHz (802.11ax R2) | 5GHz (802.11a/n/ac/ax) | 2.4GHz (802.11b/g/n/ax)
Frequency band | FCC: 5.925GHz-7.125GHz EU: 5925GHz- 6.425GHz (dependent on country) | 5.15GHz - 5.895GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM | CCK, DQPSK, DBPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM
Wireless Medium | 6-7GHz: Orthogonal Frequency Division Multiple Access (OFDMA) | 5GHz UNII: Orthogonal Frequency Division Multiple Access (OFDMA) | 2.4GHz ISM: Orthogonal Frequency Division Multiple Access (OFDMA)
Channels | All channels as defined by the relevant specification and country rules.
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ax Data Rates | Up to 2.4 Gbps
IEEE 802.11ac Data Rates | Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps

## Intel® Wi-Fi 7 BE200 (BE200NGW/BE200D2W)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.4 mm [1.5 mm max (top side)/ 0.1 mm max (bottom side)] M.2 1216: 12 mm x 16 mm x 1.7(±0.1) mm
Weight | M.2 2230: 3.07 (±0.15) g M.2 1216: 0.75 (±0.04) g
Radio ON/OFF Control | Supported
Connector Interface | M.2: PCIe*, USB
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 °C to 35 °C)
Operating Systems | Microsoft Windows 11*, Microsoft Windows 10*, Linux*
Wi-Fi Alliance* certification | Wi-Fi 7 Technology support, Wi-Fi CERTIFIED* 6 with Wi-Fi 6E, Wi-Fi CERTIFIED* a/b/g/n/ac, WMM*, WMM-PS*, WPA3*, PMF*, Wi-Fi Direct*, Wi-Fi Agile Multiband*, and Wi-Fi Location R2 HW readiness
IEEE WLAN Standard | IEEE 802.11-2020 and select amendments (selected feature coverage) IEEE 802.11a, b, d, e, g, h, i, k, n, r, u, v, w, ac, ax, be; Fine Timing Measurement based on 802.11-2016 Wi-Fi Location R2 (802.11az) HW readiness
Bluetooth | Bluetooth* 5.4
Security
Authentication | WPA3* personal and enterprise WPA2* transition mode
Authentication Protocols | 802.1X EAP-TLS, EAP-TTLS/MSCHAPv2, PEAPv0/EAP-MSCHAPv2 (EAP-SIM, EAP-AKA, EAP-AKA')
Encryption | 128-bit AES-CCMP, 256-bit AES-GCMP
Compliance
Regulatory | For a list of country approvals, please contact your local Intel representatives.
US Government | FIPS 140-3
Product Safety | UL, C-UL, CB (IEC 60950-1)
Model Numbers
Models | BE200NGW | Wi-Fi 7, 2x2, Bluetooth* 5.4, M.2 2230
BE200D2W | Wi-Fi 7, 2x2, Bluetooth* 5.4, M.2 1216
Frequency Modulation | 6-7GHz (802.11ax R2) (802.11be) | 5GHz (802.11a/n/ac/ax) | 2.4GHz (802.11b/g/n/ax)
Frequency band | FCC: 5.925GHz-7.125GHz EU: 5925GHz- 6.425GHz (dependent on country) | 5.15GHz - 5.895GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM, 4K-QAM (4096-QAM) | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM | CCK, DQPSK, DBPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM
Wireless Medium | 6-7GHz: Orthogonal Frequency Division Multiple Access (OFDMA) | 5GHz UNII: Orthogonal Frequency Division Multiple Access (OFDMA) | 2.4GHz ISM: Orthogonal Frequency Division Multiple Access (OFDMA)
Channels | All channels as defined by the relevant specification and country rules.
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ax Data Rates | Up to 2.4 Gbps
IEEE 802.11ac Data Rates | Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps

## Intel® Wi-Fi 7 BE201 (BE201NGW/BE201D2W)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.42 mm (max) M.2 1216: 12 mm x 16 mm x 1.7(±0.1) mm
Weight | M.2 2230: 3.06 (±0.14) g M.2 1216: 0.73 (±0.02) g
Radio ON/OFF Control | Supported
Connector Interface | M.2: CNVio3
Operating Temperature (Ambient) | 0 to +50 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 °C to 35 °C)
Operating Systems | Microsoft Windows 11*, Microsoft Windows 10*, Linux*
Wi-Fi Alliance* certification | Wi-Fi 7 Technology support, Wi-Fi CERTIFIED* 6 with Wi-Fi 6E, Wi-Fi CERTIFIED* a/b/g/n/ac, WMM*, WMM-PS*, WPA3*, PMF*, Wi-Fi Direct*, Wi-Fi Agile Multiband*, and Wi-Fi Location R2 HW readiness
IEEE WLAN Standard | IEEE 802.11-2020 and select amendments (selected feature coverage) IEEE 802.11a, b, d, e, g, h, i, k, n, r, u, v, w, ac, ax, be; Fine Timing Measurement based on 802.11-2016 Wi-Fi Location R2 (802.11az) HW readiness
Bluetooth | Bluetooth* 5.4 (Ant. 1)
Security
Authentication | WPA3* personal and enterprise WPA2* transition mode
Authentication Protocols | 802.1X EAP-TLS, EAP-TTLS/MSCHAPv2, PEAPv0/EAP-MSCHAPv2 (EAP-SIM, EAP-AKA, EAP-AKA')
Encryption | 128-bit AES-CCMP, 256-bit AES-GCMP
Compliance
Regulatory | For a list of country approvals, please contact your local Intel representatives.
US Government | FIPS 140-3
Product Safety | UL, C-UL, CB (IEC 62368-1)
Model Numbers
Models | BE201NGW | Wi-Fi 7, 2x2, Bluetooth* 5.4, M.2 2230
BE201D2W | Wi-Fi 7, 2x2, Bluetooth* 5.4, M.2 1216
Frequency Modulation | 6-7GHz (802.11ax R2) (802.11be) | 5GHz (802.11a/n/ac/ax) | 2.4GHz (802.11b/g/n/ax)
Frequency band | FCC: 5.925GHz-7.125GHz EU: 5925GHz- 6.425GHz (dependent on country) | 5.15GHz - 5.895GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM, 4K-QAM (4096-QAM) | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM | CCK, DQPSK, DBPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM
Wireless Medium | 6-7GHz: Orthogonal Frequency Division Multiple Access (OFDMA) | 5GHz UNII: Orthogonal Frequency Division Multiple Access (OFDMA) | 2.4GHz ISM: Orthogonal Frequency Division Multiple Access (OFDMA)
Channels | All channels as defined by the relevant specification and country rules.
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ax Data Rates | Up to 2.4 Gbps
IEEE 802.11ac Data Rates | Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps

## Intel® Wi-Fi 7 BE202 (BE200NGW M/BE200D2W M)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.4 mm [1.5 mm max (top side)/ 0.1 mm max (bottom side)] M.2 1216: 12 mm x 16 mm x 1.7(±0.1) mm
Weight | M.2 2230: 2.83 (±0.3) g M.2 1216: 0.67 (±0.1) g
Radio ON/OFF Control | Supported
Connector Interface | M.2: PCIe*, USB
Operating Temperature (Adapter Shield) | 0 to +80 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 °C to 35 °C)
Operating Systems | Microsoft Windows 11*, Microsoft Windows 10*, Linux*
Wi-Fi Alliance* certification | Wi-Fi 7 Technology support, Wi-Fi CERTIFIED* 6 with Wi-Fi 6E, Wi-Fi CERTIFIED* a/b/g/n/ac, WMM*, WMM-PS*, WPA3*, PMF*, Wi-Fi Direct*, Wi-Fi Agile Multiband*, and Wi-Fi Location R2 HW readiness
IEEE WLAN Standard | IEEE 802.11-2020 and select amendments (selected feature coverage) IEEE 802.11a, b, d, e, g, h, i, k, n, r, u, v, w, ac, ax, be; Fine Timing Measurement based on 802.11-2016 Wi-Fi Location R2 (802.11az) HW readiness
Bluetooth | Bluetooth* 5.4
Security
Authentication | WPA3* personal and enterprise WPA2* transition mode
Authentication Protocols | 802.1X EAP-TLS, EAP-TTLS/MSCHAPv2, PEAPv0/EAP-MSCHAPv2 (EAP-SIM, EAP-AKA, EAP-AKA')
Encryption | 128-bit AES-CCMP, 256-bit AES-GCMP
Compliance
Regulatory | For a list of country approvals, please contact your local Intel representatives.
US Government | FIPS 140-3
Product Safety | UL, C-UL, CB (IEC 60950-1)
Model Numbers
Models | BE200NGW M | Wi-Fi 7, 160MHz 2x2, Bluetooth* 5.4, M.2 2230
BE200D2W M | Wi-Fi 7, 160MHz 2x2, Bluetooth* 5.4, M.2 1216
Frequency Modulation | 6-7GHz (802.11ax R2) (802.11be) | 5GHz (802.11a/n/ac/ax) | 2.4GHz (802.11b/g/n/ax)
Frequency band | FCC: 5.925GHz-7.125GHz EU: 5925GHz- 6.425GHz (dependent on country) | 5.15GHz - 5.895GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM, 4K-QAM (4096-QAM) | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM | CCK, DQPSK, DBPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM
Wireless Medium | 6-7GHz: Orthogonal Frequency Division Multiple Access (OFDMA) | 5GHz UNII: Orthogonal Frequency Division Multiple Access (OFDMA) | 2.4GHz ISM: Orthogonal Frequency Division Multiple Access (OFDMA)
Channels | All channels as defined by the relevant specification and country rules.
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ax Data Rates | Up to 2.4 Gbps
IEEE 802.11ac Data Rates | Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps

## Intel® Wi-Fi 7 BE211 (BE211NGW/BE211D2W)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.42 mm M.2 1216: 12 mm x 16 mm x 1.7(±0.1) mm
Weight | M.2 2230: 3.06 (±0.14) g M.2 1216: 0.73 (±0.02) g
Radio ON/OFF Control | Supported
Connector Interface | M.2: CNVio3
Operating Temperature (Ambient) | 0 to +50 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 °C to 35 °C)
Operating Systems | Microsoft Windows 11*, Microsoft Windows 10*, Linux*
Wi-Fi Alliance* certification | Wi-Fi 7 Technology support, Wi-Fi CERTIFIED* 6 with Wi-Fi 6E, Wi-Fi CERTIFIED* a/b/g/n/ac, WMM*, WMM-PS*, WPA3*, PMF*, Wi-Fi Direct*, Wi-Fi Agile Multiband*, and Wi-Fi Location R2 HW readiness
IEEE WLAN Standard | IEEE 802.11-2020 and select amendments (selected feature coverage) IEEE 802.11a, b, d, e, g, h, i, k, n, r, u, v, w, ac, ax, be; Fine Timing Measurement based on 802.11-2016 Wi-Fi Location R2 (802.11az) HW readiness
Bluetooth | Bluetooth* 5.4
Security
Authentication | WPA3* personal and enterprise WPA2* transition mode
Authentication Protocols | 802.1X EAP-TLS, EAP-TTLS/MSCHAPv2, PEAPv0/EAP-MSCHAPv2 (EAP-SIM, EAP-AKA, EAP-AKA')
Encryption | 128-bit AES-CCMP, 256-bit AES-GCMP
Compliance
Regulatory | For a list of country approvals, please contact your local Intel representatives.
US Government | FIPS 140-3
Product Safety | UL, C-UL, CB (IEC 60950-1)
Model Numbers
Models | BE211NGW | Wi-Fi 7 R2, 2x2, Bluetooth® Core Spec 6.0, M.2 2230
BE211D2W | Wi-Fi 7 R2, 2x2, Bluetooth® Core Spec 6.0, M.2 1216
Frequency Modulation | 6-7GHz (802.11ax R2) (802.11be) | 5GHz (802.11a/n/ac/ax) | 2.4GHz (802.11b/g/n/ax)
Frequency band | FCC: 5.925GHz-7.125GHz EU: 5925GHz- 6.425GHz (dependent on country) | 5.15GHz - 5.895GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM, 4K-QAM (4096-QAM) | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM | CCK, DQPSK, DBPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM
Wireless Medium | 6-7GHz: Orthogonal Frequency Division Multiple Access (OFDMA) | 5GHz UNII: Orthogonal Frequency Division Multiple Access (OFDMA) | 2.4GHz ISM: Orthogonal Frequency Division Multiple Access (OFDMA)
Channels | All channels as defined by the relevant specification and country rules.
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ax Data Rates | Up to 2.4 Gbps
IEEE 802.11ac Data Rates | Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps

## Intel® Wi-Fi 7 BE213 (BE211NGW M/BE211D2W M)

General
Dimensions (H x W x D) | M.2 2230: 22 mm x 30 mm x 2.42 mm M.2 1216: 12 mm x 16 mm x 1.7(±0.1) mm
Weight | M.2 2230: 3.06 (±0.14) g M.2 1216: 0.73 (±0.02) g
Radio ON/OFF Control | Supported
Connector Interface | M.2: CNVio3
Operating Temperature (Ambient) | 0 to +50 degrees Celsius
Humidity | 50% to 90% RH non-condensing (at temperatures of 25 °C to 35 °C)
Operating Systems | Microsoft Windows 11*, Microsoft Windows 10*, Linux*
Wi-Fi Alliance* certification | Wi-Fi 7 Technology support, Wi-Fi CERTIFIED* 6 with Wi-Fi 6E, Wi-Fi CERTIFIED* a/b/g/n/ac, WMM*, WMM-PS*, WPA3*, PMF*, Wi-Fi Direct*, Wi-Fi Agile Multiband*, and Wi-Fi Location R2 HW readiness
IEEE WLAN Standard | IEEE 802.11-2020 and select amendments (selected feature coverage) IEEE 802.11a, b, d, e, g, h, i, k, n, r, u, v, w, ac, ax, be; Fine Timing Measurement based on 802.11-2016 Wi-Fi Location R2 (802.11az) HW readiness
Bluetooth | Bluetooth* 6.0
Security
Authentication | WPA3* personal and enterprise WPA2* transition mode
Authentication Protocols | 802.1X EAP-TLS, EAP-TTLS/MSCHAPv2, PEAPv0/EAP-MSCHAPv2 (EAP-SIM, EAP-AKA, EAP-AKA')
Encryption | 128-bit AES-CCMP, 256-bit AES-GCMP
Compliance
Regulatory | For a list of country approvals, please contact your local Intel representatives.
US Government | FIPS 140-3
Product Safety | UL, C-UL, CB (IEC 60950-1)
Model Numbers
Models | BE211NGW M | Wi-Fi 7 R2, 2x2, Bluetooth® Core Spec 6.0, M.2 2230
BE211D2W M | Wi-Fi 7 R2, 2x2, Bluetooth® Core Spec 6.0, M.2 1216
Frequency Modulation | 6-7GHz (802.11ax R2) (802.11be) | 5GHz (802.11a/n/ac/ax) | 2.4GHz (802.11b/g/n/ax)
Frequency band | FCC: 5.925GHz-7.125GHz EU: 5925GHz- 6.425GHz (dependent on country) | 5.15GHz - 5.895GHz (dependent on country) | 2.400 - 2.4835GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM | BPSK, QPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM | CCK, DQPSK, DBPSK, 16 QAM, 64 QAM, 256 QAM, 1024 QAM
Wireless Medium | 6-7GHz: Orthogonal Frequency Division Multiple Access (OFDMA) | 5GHz UNII: Orthogonal Frequency Division Multiple Access (OFDMA) | 2.4GHz ISM: Orthogonal Frequency Division Multiple Access (OFDMA)
Channels | All channels as defined by the relevant specification and country rules.
Data Rates | All data rates are theoretical maximums.
IEEE 802.11ax Data Rates | Up to 2.4 Gbps
IEEE 802.11ac Data Rates | Up to 867 Mbps
IEEE 802.11n Data Rates | Tx/Rx (Mbps): 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps

Back to Top

Back to Contents

Trademarks and Disclaimers